{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Sheet1","Sheet2"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":23,"n_cols":10,"rows_kept":23,"merged":[[0,0,0,9],[18,0,18,1],[18,2,18,7],[19,0,19,1],[19,2,19,7],[20,0,20,1],[20,2,20,7],[21,0,21,1],[21,2,21,7],[22,0,22,9]],"flags":["formulas_cached_only"]}
["安康学院校园监控系统增容工程设备招标采购清单"]
["序号","设备名称","品牌","参考型号","规格","单位","数量","单价(元)","金额(元)","备注"]
[1,"硬盘录像机",null,"DS-8016","可接全球眼平台","台",1]
[2,"硬盘 ",null,null,"1TB","块",1]
[3,"操控台",null,null,"单联钢制","台",1]
[4,"云台控制键盘",{"$nulls":3},"台",1]
[5,"视频切换矩阵",null,null,"16路","台",1]
[7,"监视器",null,null,"21寸彩色","台",1,null,null,"电视墙使用"]
[8,"全方位旋转变焦摄像机",null,"7413A","1/4英寸Super-HAD IT CCD；600线；25倍(f=3.4～85mm) 光学；16倍(0.1step)\n数字变焦；最低照度：彩色0.001 Lux ；黑白 0.0001 Lux ；0～360度水平连续旋转； 0～180度垂直翻转","台",3]
[9,"云台支架",{"$nulls":3},"个",3,null,null,"配套全方位旋转变焦摄像机使用"]
[10,"半球摄像机",null,"5366A","1/3英寸Super HAD IT CCD；600线；0.00023Lux","台",7,null,null,"室内监控、顶部安装"]
[11,"枪式摄像机",null,"2031A","1/3英寸Super-HAD IT CCD；600线；彩色0.12Lux,黑白0.012Lux","台 ",3,null,null,"过道、食堂等通道监控"]
[12,"摄像机支架护罩",{"$nulls":3},"套",3,null,null,"配套枪式摄像机用"]
[13,"8路多业务光端机",null,"烽火机架式","含机架及电源","台",2]
[14,"单路多业务光端机",null,"烽火台式",null,"台",13]
[15,"综合设备箱",null,null,"含有插座，终端盒、尾纤、空开等配件","套",13,null,null,"安放光端机、终端盒等设备"]
[16,"光缆",null,null,"12芯","KM",3,null,null,"视频传输线缆"]
[17,"线缆、线管、接头等辅材",{"$nulls":3},"套",13]
["设备合计"]
["安装调试费"]
["税金"]
["工程总计"]
["说明：公布的产品型号为参考型号，非指定性要求，设备性能达到或优于参考型号产品性能均可。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}