{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":14,"n_cols":10,"rows_kept":14,"merged":[[0,0,0,9]],"flags":["formulas_cached_only"]}
["安康学院蚕桑重点实验室仪器设备采购清单"]
["序号","仪器名称","品牌","参考型号","规格","单位","数量","参考单价(元）","金额(元）","备注"]
[1,"移液器",null,null,"0.5-10μl/BP10；\n5-50μl/BP50；\n20-200μl/BP200；\n100-1000μl/BP1000","套",1,null,null,"每种型号各1把，共4把"]
[2,"冷藏柜",null,"LC-122A ","容积: 122L","台",1]
[3,"酸度计",null,"PHS-3C","3 1/2位LED数字显示；E-201-C型pH复合电极；具3点校正功能；测量范围： pH：0~14.00；温度补偿范围：0~60℃；电子单元基本误差：±0.01 pH；电子单元输入电流不大于2×10-12A，输入阻抗：不小于 l×1012Ω；重复性误差：不大于0.01 pH","台",1]
[4,"控温摇床",null,null,"可摇1L、500ml、250ml和100ml三角瓶；\n摇床温度可控；具加热和制冷系统；温度范围：5-50℃；工作尺寸：82*52cm；屏显控制系统；配相应配件各一套；","台",1]
[5,"PCR基因扩增仪",null,"ABI 2720型","1. 记忆功能：可储存100个方法（包括PCR前处理，PCR循环，PCR后处理）；2. 显示屏：A7*40字节可显示倒计时时间和已完成循环数，闪烁图形提示温度变化当前状态；3. 可编程序：可任意修改预设的程序（包括前处理，后处理和25个循环）；设定好的程序可以储存并可以加密保护防止无意改写；4. 软件功能：循环时间和温度自动延伸/自动下降，可停程序；有时间日期显示，自动断电保护，恢复供电后自动执行未完成循环，保证扩增过程安全运行；计算Tm值，温度验证功能 ；5. 用户自检：用户可常规运行多种诊断程序以检测仪器升降温速度和升降温精度 ；6. 温度范围：4.0-99.9℃ ；7. 温度显示：仪器显示经计算机计算的实际样品温度，精确到0.1℃；8. 实际样品的平均升/降温速度： 1℃/秒 ；9. 样品基座升降温速度： 2.7℃/秒 ；10. 静态样品基座温度均匀性： ±0.5℃，95℃计时后30秒 ；11. 温度准确性：正负0.5℃，35 －100℃范围 ；12. 温度校正：符合美国国家标准技术局标准（NIST）；13. 热盖：维持105℃温度，满足无油操作PCR扩增 ；14. 重现性：达到设定温度的时间误差小于5秒。","台",1]
[6,"人工气候箱",null,"SPX-250IC","容积：250L；微电脑普通型；控温范围：5-50℃（有光照时） 0-50℃（无光照时）；温度波动±1℃；控湿范围：50%-95%；湿度波动±5%；光照强度：0-15000LX（五级可调）；载物托架标配（4块）","台",1]
[7,"稳压稳流器",null,null,"输出功率2kw以上","台",3]
[8,"检尺器",null,"YG731","1.125米；100回或100回的倍数；","台",2]
[9,"潘通色卡",null,null,"3位","套",1]
[9,"潘通色卡",null,null,"6位","套",1]
[10,"人工气候箱",null,"HPG-320H","四面光照；LED显示；总容积：320L；\n0～9000Lx分五级可调 0～9000Lx分五级可调；温度范围 有光照  10-50℃；无光照 5-50℃；温度波动性 ±0.5℃ ；温度均匀性 ±1.0℃ ；温度调节范围 95%以下；\n两个温度设定功能：可随光照的有无实现昼夜变化的两个温度，光的强度可分级凋节；\n采用干、湿球双温控制法调节箱内温、湿度，并分别显示；低温补偿功能；不锈钢内胆。","台",1]
["小计"]