{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["第一标段","第二标段","第三标段","第四标段"],"not_rendered":{"external_links":1,"defined_names":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"第一标段","index":0,"n_rows":11,"n_cols":10,"rows_kept":11,"merged":[[0,0,0,9],[1,0,1,9]],"flags":["formulas_cached_only"]}
["安康学院电子与信息工程系实验室仪器设备采购清单"]
["第一标段：DSP/SOPC实验室设备"]
[]
["序号","设备名称","品牌","参考型号","规格","单位","数量","单价(元)","金额(元)","备注"]
[1,"DSP实验开发系统",null,"ZY11301D","DSP开发系统主板：\n1、核心主板包含3万门的FPGA；2、接口资源丰富，如USB2.0接口、以太网接口、PS/2键盘接口、VGA显示接口等。3、数码管模块：采用8位数码管，可以利用DSP控制LED做数据显示，也可以直接利用FPGA来控制LED做数字钟的实验项目。4、LCD模块：采用122×32的图形液晶模块，可用DSP来控制LCD做图形显示，也可利用FPGA直接来控制LCD。5、UART模块：采用异步RS232串口。6、开关量输入输出模块：采用轻触按键、双刀双掷开关、拨码开关来作为逻辑输入，逻辑输出采用16位LED。7、PS/2键盘输入模块：可以接标准键盘。8、信号调理模块：对信号进行叠加和放大。9、滤波模块：对信号进行模拟滤波。10、提供MATLAB与DSP的接口。\n  附件：1、54XEVM板(DSP扩展板)。2、ZY11301D-voice语音卡；\n3、ZY11301D-ethernet以太网卡；4、ZYUSB2.0 EMULATOR USB2.0仿真器；5、开发软件和教学资源光盘。","套",32]
[2,"SOPC开发板(主板)",null,"DE2-70 Development and Education Board","The DE2-70 box includes:\n*The 8 x 6 inch DE2-70 board with a Cyclone II EP2C70 (896-pin package) FPGA;* 12V AC/DC adaptor;* USB cable;* Plexiglas cover for the DE2-70 boar;* 64 MB SDRAM, 2 MB SSRAM, 8 MB Flash;* SD memory card slot;* Eight 7-segment displays;* 16 x 2 LCD display;* 18 toggle switches;* 18 red LEDs* 9 green LEDs;* Four debounced pushbutton switches;* 50 MHz clock* 27 MHz clock;* External SMA clock input ;  \nSoftware : Quatus II and Nois II.","套",32]
[3,"SOPC开发板500万像素数字相机附件",null,"Altera 500万像素数字相机套件","* Complete reference design with source code in Verilog HDL.\n* Support exposure time controlling - users can adjust the exposure according to the light of the surrounding area* Support motion capture mode;* Software allows users to upload the picture captured into PC and save the picture into bitmap format or Joint Photographic Experts Group for viewing;* Equipped with Micron 5 Mega Pixel CMOS sensor;* Provide users entire reference design (Frame Grabber, high-performance multi-port SDRAM frame buffer, image processing IPs);* Support Altera DE3/ DE2_70/ DE2/ DE1/DE0 and Cyclone II Starter boards.   \n * Size：78*59.5 mm","套",16]
[4,"SOPC开发板4.3\" LCD 触碰面板附件",null,"Altera 4.3\" LCD 触碰面板套件","*The 4.3\" Ultra-high Resolution LCD Touch Panel Development Kit provides users a 800x480 full-color high-quality LCD Touch Panel with complete reference designs and source code allowing users to develop applications by a touch panel on the Altera DE3/DE2-70/DE2/DE1/DE0 board and Altera Cyclone II Starter Kit.  * Support Altera DE3/ DE2_70/ DE2/ DE1/DE0 and Cyclone II Starter boards. \n * Size：127*87 mm","套",16]
[5,"SOPC开发板AD /DA子板",null,"Altera AD/DA子板","* 双AD通道提供14位分辨率和高达65 MSPS的传输速率;* 双DA通道提供，14位分辨率和高达125 MSPS的传输速率;* 提供HSMC和GPIO双接口,可兼容于 Cyclone III入门套件或DE0/DE1/DE2/DE3 开发套件系列;* 时脉来源可以来自100MHz振荡器 、AD/DA通道的SMA接口、HSMC/GPIO接口上的PLL界面  * 尺寸：90.3*78.2毫米","套",16]
[6,"Altera Nios II 高阶多媒体嵌入式(SOPC)开发套件",null,"Altera Nios II 高阶多媒体嵌入式系统开发套件","* LCD daughtercard（Color LCD touch-screen display + 800 x 480 resolution；24-bit CD-quality Audio CODEC with line-in, line-out, and microphone-in jacks；10/100 Ethernet physical layer/media access control；Connectors）  *The Cyclone III FPGA Starter Kit（Cyclone III EP3C25F324 FPGA；32 Mbytes of DDR SDRAM；50-MHz, on-board oscillator；Seven LEDs total, four user controlled；128-Mbyte SD card and USB-to-SD card adapter；etc.)  * Nios II Evaluation kit CD-ROM（Hardware tutorials;Software tutorials;Complete document）  * Altera Complete Design Suite DVD (Free);","套",2]
[null,"合计"]

{"sheet":"第二标段","index":1,"n_rows":19,"n_cols":10,"rows_kept":19,"merged":[[0,0,0,9],[1,0,1,9],[2,0,2,9],[11,0,11,2],[12,0,12,9],[17,0,17,2],[18,0,18,2]],"flags":["formulas_cached_only"]}
["安康学院电子与信息工程系实验室仪器设备采购清单"]
["第二标段：嵌入式（ARM）实验室及电子开放实验室设备"]
["一、嵌入式（ARM）实验室"]
["序号","设备名称","品牌","参考型号","规格","单位","数量","单 价(元)","金 额(元)","备注"]
[1,"ARM双核实验系统",null,"ARM9/ARM10  UP-CUP S2410/P270","平台为ARM9和XSCALE双核平台，通过更换核心板即可满足嵌入式教学、科研的两种要求，实现完全兼容。可以运行Linux、WinCE、μC/OS-Ⅱ、Vxworks四种操作系统。基本配置为XSCALE核心板，可根据需要选配若干ARM9核心板。该平台为中国电子学会嵌入式认证考试指定平台。\n附件：开发工具：EWARM-BL-NW（网络版）","套",32,null,null,"（同时配备三星公司 S3C2410核心板和Intel公司 PXA270核心板）"]
[2,"ARM实验系统扩展块",null,"3种扩展模块组","传感器扩展板模块、ZigBee应用套件、智能语音识别套件。","套",16]
[3,"嵌入式大屏幕实训系统",null,"UP-LED大屏幕实训系统","*基于ARM控制和CPLD扫描方案的LED大屏幕控制器* CPLD时序逻辑独立驱动LED带来稳定的显示效果* 开放的ARM应用程序开发框架，实现字库操作、显示效果和通信功能* 支持多种分辨率和拼装方式* 双色屏分辨率为1024×32点* 尺寸：256cm×128cm* 具有可扩展性；","套",1]
[4,"嵌入式“魔法师”创意实训套件",null,"UP-Magic“魔法师”创意实训套件","该套件是一套用于开展嵌入式技术创新实验的模块化实训套件，以ARM9处理器S3C2410最小系统为核心，通过核心板和底板上的各种接口进行扩展，具有多种类配套模块可选购。具体包括：主控板单元、通讯类模块、输入/输出类模块、传感器类模块、功能扩展类模块以及相应的配线等。（“魔法师”创意实训套件的总体外观一改市面上嵌入式系统开发板结构单一的风格，而是由处理器核心板和数十种基本“积木”构件的标准模块、面包板、连接电缆等组成。用这些模块可以搭建出各种嵌入式应用原型，为学生学习嵌入式技术、进行课程设计和实践训练提供了空前的灵活性，是当前嵌入式技术教学中实训环节的优质教材。在套件使用过程中，除采用既有模块外，学生还可自由发挥进行创意设计，亲自动手，体验魔法师的乐趣。）","套",5]
[5,"单片机小系统开发板",null,"HC6800V2.6","增强型STC89C52单片机小系统板，系统板载：2个4位共阴极数码管、1位共阳数码管、4*3矩阵键盘、八个独立按钮、8路显示LED、74HC595驱动、双色8*8LED点阵、蜂铃器、RTC实时时钟DS1302、工业级AD/DA转换IC、A24C02(EEPROM)、LS138译码器、达林顿ULN2003驱动芯片、MAX232串口、输出继电器、实时时钟（PCF8563）、USB接口（供电、通信、烧录程序、仿真等功能）。\n附件：步进电机、直流电机、红外接收头、外遥控器、1602液晶屏、18B20温度检测器、八位排线、单P杜邦线、GUIBuilder工业组态软件、DVD教学光盘（含KeivuV2视频教程、单片机视频教程、C语言视频教程）、铝镁合金箱等。","套",32]
[6,"数字示波器","固纬/泰克/安捷伦",null,"Bandwidth：DC~60MHz(-3dB);Rise Time：<5.8ns Approx；Sensitivity：2mV/div ~ 10V/div (1-2-5 increments)；Accuracy：±(3% x |Readout| + 0.1 div + 1mV)；Input Coupling：AC, DC & Ground；Input Impedance：1MΩ±2%, ~15pF；Maximum Input：300V (DC+AC peak), CATII；Waveform Signal Process：+ , - , x, FFT, FFTrms；Bandwidth Limit：20MHz (-3dB)；Real-Time Sample Rate：1GSa/s maximum","台",16,null,null,"从三个备选品牌中选择一个进行报价"]
[7,"数字万用表",null,"UT60E","功能：直流电压\\交流电压\\直流电流\\交流电流\\电阻\\电容\\频率\\温度\\占空比\\真效值\\二极管测试\\通断蜂鸣\\全符号显示\\低电压提示\\电压测量\\数据保持\\RS232接口\\自动手动量程选择\\背光\\睡眠；\n附件：表笔，点式温度探头，电池，说明书，测试夹，保修卡，标准，RS232电脑接线，测试软件","台",32]
["小计"]
["二、电子开放实验室"]
[1,"数字示波器","固纬/泰克/安捷伦",null,"Bandwidth：DC~60MHz(-3dB);Rise Time：<5.8ns Approx； Sensitivity：2mV/div ~ 10V/div (1-2-5 increments)；Accuracy：±(3% x |Readout| + 0.1 div + 1mV)；Input Coupling：AC, DC & Ground；Input Impedance：1MΩ±2%, ~15pF；Maximum Input：300V (DC+AC peak), CATII；Waveform Signal Process：+ , - , x, FFT, FFTrms；Bandwidth Limit：20MHz (-3dB)；Real-Time Sample Rate：1GSa/s maximum","台",20,null,null,"从三个备选品牌中选择一个进行报价"]
[2,"四路直流电源",null,"MPS-3002L-3","双路0-30V/0-2A 连续可调，双路5V/2A 固定输出，4路输出。","台",20]
[3,"信号发生器",null,"UT9003A","0.1Hz-3MHz，正弦、方波，三角波，升斜坡，降斜坡、升指数、降升指数；测频范围：1Hz～100MHz.","台",20]
[4,"电工工具",null,null,"尖嘴钳、斜口钳、剥线钳、十字、一字螺丝刀、烙铁架、烙铁、电热吸锡器、镊子、小剪刀、UT39B万用表、工具箱","套",20]
["小计"]
["总计"]

{"sheet":"第三标段","index":2,"n_rows":9,"n_cols":10,"rows_kept":9,"merged":[[0,0,0,9],[1,0,1,9],[5,0,5,3],[8,0,8,9]],"flags":["formulas_cached_only"]}
["安康学院电子与信息工程系实验室仪器设备采购清单"]
["第三标段：实验台设备"]
[]
["序号","设备名称","品牌","参考型号","规格","单位","数量","单 价(元)","金 额(元)","备注"]
[1,"实验台",null,"双座","1、规格实验桌：长1800×宽800×高（750+500）mm。2、实验仪器面：长1800宽×350×25mm上表面靠后有四个电源孔方便连线，后面有20-100mm(根据实用性和美观性选择)挡板防止仪器后移；3、钢板制电源箱，表面静电喷涂，电器配漏电保护开关，12孔多用插座，指示灯，电脑用插座开关（独立电源和实验台保护开关不相连）；4、实验台面与实验仪器面高距500mm；5、实验台面：长1800×宽800×高25mm防火板台面，上表面有2个电源孔下面有ABC键盘托（两个在两边）；刚板抽屉（1个中间），表面静电喷涂；6、铝型材立柱表面电化处理；7、钢管框架静电喷涂；8、钢管主机箱吊架静电喷涂与实验台底面和内侧立柱相连（两边各一个）；9、钢管腿静电喷涂配可调节地脚；10、实验仪器面下安装操作灯管；附件：方凳2个。","套",25,null,null,"要求生产厂家提供设计图纸及相关说明材料"]
["合计"]
[]
[]
["要求系上提供示意图。"]

{"sheet":"第四标段","index":3,"n_rows":7,"n_cols":10,"rows_kept":7,"merged":[[0,0,0,9],[1,0,1,9],[2,0,2,9],[6,0,6,1]],"flags":["formulas_cached_only"]}
["安康学院电子与信息工程系实验室仪器设备采购清单"]
["第四标段：计算机及投影设备"]
["一、电子信息工程系实验室"]
["序号","设备名称","品牌","参考型号","规格","单位","数量","单 价(元)","金 额(元)","备注"]
[1,"计算机","联想/惠普/戴尔（商用系列）",null,"Intel 奔腾双核 E5400(2.7G)、2G内存、320G硬盘(7200转)、19英寸显示器(LCD)、DVD-ROM光驱、独显(512MB)、1000Mbps以太网卡、立式机箱、windows XP professional、Redhat操作系统等。","台",70,null,null,"从三个备选品牌中选择一个进行报价"]
[2,"教育投影机","爱普生/三菱/索尼",null,"显示技术：3LCD；亮度：3500流明；对比度600:1；标准分辨率：1024×768dpi；最高分辨率1600×1200dpi；投影光源：超高压汞灯；投影方式：正投；投影画面尺寸：30-300英寸；投影灯泡寿命不小于5000小时。\n  附件：2-4口VGA分频器；电动玻珠幕布、150英寸；","台",2,null,null,"从三个备选品牌中选择一个进行报价"]
["小计"]