{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["第一标段 ","第二标段","第三标段","第四标段"],"not_rendered":{"external_links":1,"defined_names":15},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"第一标段 ","index":0,"n_rows":17,"n_cols":10,"rows_kept":17,"merged":[[0,0,0,9],[1,0,1,9],[16,0,16,1]],"flags":["formulas_cached_only"]}
["安康学院教学仪器设备采购清单"]
["第一标段：电子技术实验室设备"]
["序号","仪器名称","品牌","型号","规格","单位","数量","单价(元）","金额(元）","备注"]
[1,"数字双踪示波器",null,"UT2102CE","双踪60MHz，彩色LCD屏幕，采样率1GSa/s","台",30]
[2,"数字合成信号发生器",null,"UT9003A","0.1Hz-3MHz，正弦、方波，三角波，升斜坡，降斜坡、升指数、降升指数；测频范围：1Hz～100MHz.","台",30]
[3,"直流稳压电源",null,"XJ17432","双路0-30V/0-2A 连续可调，双路5V/2A 固定输出，4路输出。","台",30]
[4,"ARM/DSP嵌入式实验开发系统",null,"精益达盛EL-ARM/DSP-IV","DSP+ARM设计结构。","套",3]
[5,"电子竞赛板",null,"KX-DVP3F","FPGACycloneII FPGA EP2C8，40万门；isp单片机AT89S8253、PS/2键盘接口、USB接口、VGA接口、RS232串口；高速ADC/DAC板：180MHz转换率双路高速10位DAC、50MHz高速8位ADC、双300MHz高速运放。","套",5]
[6,"自主创新综合实验开发系统",null,"KX_DSN3","MCS-51单片机模块、可运行单片机IP核的FPGA模块（实现SOPC设计）、点阵型液晶显示屏、字符型液晶显示屏、A/D与D/A模块、VGA显示接口模块、语音录放模块、无线遥控编码收发模块、DDS模块等。","套",5]
[7,"实验桌凳",null,null,"长1800×宽800×高（750+600），钢木结构，漏电保护，防火阻燃（橡胶垫），抽屉，电源指示灯，电源插座，搁物板（放置仪器），放2台计算机主机和显示器。","套",15]
[8,"仪器桌",null,null,"长1600×宽800×高750，钢木结构、铁制抽屉，带电源座","套",6]
[9,"电子技术实验板",null,null,"400×310×120mm，带电源及信号输入和输出接线柱（口），耐用有垫脚。","套",30]
[10,"电子工具",null,null,"尖嘴钳、斜口钳、剥线钳、十字、一字螺丝刀、烙铁架、烙铁、电热吸锡器、镊子、小剪刀、UT39B万用表、工具箱","套",30,null,null,"学生用"]
[11,"电子工具",null,null,"MF47T万用表、拔放台、恒温焊台、尖嘴钳、斜口钳、剥线钳、螺丝批、电动吸锡器、镊子、小剪刀、板尺、工具箱","套",2,null,null,"教师用"]
[12,"常用元器件及耗材",null,null,"74系列、C4000系列、运放、常用晶体管、1/4W电阻系列、电容电感系列、焊锡丝、松香、焊膏、测试线、电位器、9V和2号电池、二、三级管等。","批",1,null,null,"根据详细清单核销"]
[13,"元器件柜",null,null,"铁制，12个斗柜，1个顶柜1个侧门柜，90长×40宽×高186cm(带锁）","个",3]
["合计"]

{"sheet":"第二标段","index":1,"n_rows":7,"n_cols":10,"rows_kept":7,"merged":[[0,0,0,9],[1,0,1,9],[6,0,6,1]],"flags":["formulas_cached_only"]}
["安康学院教学仪器设备采购清单"]
["第二标段：通信原理实验室设备"]
["序号","仪器名称","品牌","型号","规格","单位","数量","单价(元）","金额(元）","备注"]
[1,"现代通信技术创新实验系统",null,"ZY11801G","1.嵌入式模块化设计；2.能完成通信技术基础实验、创新实验以及二次开发实验；3.信号源模块含有模拟信号源、数字信号源、DDS信号源；4.用通信系统来串接通信原理中的11种关键技术，能实现五大完整的通信系统；5.含CPLD、DSP、ARM、单片机等二次开发模块；6.含GPRS模块和无线收发模块；7.核心芯片采用有机玻璃挡板保护。","套",20]
[2,"数字存储示波器",null,"UT2062CE","双踪60MHz，5.7寸彩色LCD屏幕，采样率1GS/S","台",20]
[3,"数字万用表",null,"UT60E",null,"台",20]
["合计"]

{"sheet":"第三标段","index":2,"n_rows":12,"n_cols":10,"rows_kept":12,"merged":[[0,0,0,9],[1,0,1,9],[3,9,4,9],[11,0,11,1]],"flags":["formulas_cached_only"]}
["安康学院教学仪器设备采购清单"]
["第三标段：电子与信息工程系计算机设备"]
["序号","仪器名称","品牌","型号","规格","单位","数量","单价(元）","金额(元）","备注"]
[1,"教师用计算机","DELL/联想/HP",null,"Intel 酷睿2双核 E7200/4G/250G/独立256MB显卡/19寸LCD/  DVD+/-RW/  音箱","台",2,null,null,"在所列品牌中任选一个品牌"]
[2,"学生用计算机","DELL/联想/HP",null,"Intel 酷睿2双核 E7400 2.8GHz/4G/250G/独立256MB显卡/19寸LCD","台",30]
[3,"投影机","松下/爱普生/NEC/SONY",null,"投影方式：正投/背投/LCD投影/不小于3500流明/标准分辨率1024*768/对比度 600：1/屏幕比例 16：9 、4：3/灯泡寿命不小于2000小时/可直接断电，支持工作状态读取","台",2]
[4,"投影幕布","红叶",null,"电动，白塑，150英寸","台",1]
[5,"投影幕布","红叶",null,"电动，白塑，120英寸","台",1]
[6,"笔记本电脑","DELL/联想/HP",null,"Intel 酷睿2双核 P8600（2.4GHz）/2GB/250GB/内置DVD刻录机/12.1LCD","台",3]
[7,"辅材",{"$nulls":3},"批"]
[8,"工程及其他"]
["合计"]

{"sheet":"第四标段","index":3,"n_rows":82,"n_cols":10,"rows_kept":82,"merged":[[0,0,0,9],[1,0,1,9],[3,0,3,9],[46,0,46,1],[47,0,47,9],[55,0,55,1],[56,0,56,9],[67,0,67,1],[68,0,68,9],[75,0,75,1],[76,0,76,9],[80,0,80,1],[81,0,81,1]],"flags":["formulas_cached_only"]}
["安康学院教学仪器设备采购清单"]
["第四标段：化学化工系实验室设备"]
["序号","仪器名称","品牌/厂家","型号","规格","单位","数量","单价(元）","金额(元）","备注"]
["一、材料及提取分离实验室"]
[1,"箱式电阻炉",null,"SX2-2.5-10","200×120×80,工作温度1000℃","台",1]
[2,"高温粘度测定仪",null,"GN020","300×300","台",1]
[3,"实验室粉碎磨",null,"JFSD-70","台式，四个工位，罐材料为耐磨聚氨脂、容积100ml，出料粒度0.1μm，","台 ",1]
[4,"荧光显微镜",null,"XSP-63X","三目，1600倍","台",1]
[5,"差动热分析仪",null,"CDR-1","DSC:4-100mV;DTA：10-100Uv,温度：室温-800度（含电脑、打印机）","台",1]
[6,"双数显专用拉压试验机",null,"SZL-200","国家标准WE- 300A","台",1]
[7,"电动洛氏硬度仪",null,"HR-150DT","预试验力98","台",1]
[8,"电子天平",null,"MA200","200g，0.0001g,自动显示数据","台",1]
[9,"连续变倍体视显微镜",null,"XYH03","放大倍数7X~45X","台",1]
[10,"水热反应釜",null,null,"50ml、30ml","台",10]
[11,"自动低压液相色谱分离层析仪",null,"HD005-F","台式","台",1]
[12,"循环水真空泵",null,"SHE-Ⅲ",null,"台",2]
[13,"实验微波炉",null,"MKJ-H1","0~300度红外测试仪微波功率实现无级连续调节，0~800W连续可调","台",1]
[14,"玛瑙研钵",null,null,"φ90","台",2]
[15,"旋光仪",null,"WZZ-2B","微机，数显，最小读数单位：0.005℃","台",1]
[16,"电子分析天平",null,"FA1004","100g/0.1mg","台",1]
[17,"水分测定仪",null,"SC69-02C","100g/0.1mg","台",1]
[18,"显微熔点测定仪",null,"WRS-1B","微机，数显，最小读数单位：0.1℃","台",1]
[19,"离心机",null,"HimacCF15RXII","最大容量4×250ml","台",1]
[20,"超声波清洗机",null,"HS-120D","可控温，功率1200","台",1]
[21,"玻璃色谱板",null,null,"10×10 cm，5×10 cm","个",200]
[22,"小型色谱柱",null,null,"直径：5cm /2.5","台",16]
[23,"梨形分液漏斗",null,null,"500 ml /1000 ml","台",16]
[24,"索氏提取器",null,"SXT-06","含油量在0.5%-60%范围内的各种样品","台",1]
[25,"中草药粉碎机",null,"FW177","一次投入量：400g，粉碎60-120目","台",1]
[26,"小型电动离心机",null,80,"容量：6×1.5，6×0.5","台",1]
[27,"电热恒温干燥箱",null,"202-O-S","数显","台",1]
[28,"旋转蒸发仪",null,"R501B","5升，伸降水浴锅，转速数显","台",1]
[29,"台式冷冻干燥机",null,"FD-1","普通","台",1]
[30,"智能崩解仪",null,"ZB-1C型","两杯式","台",1]
[31,"实验台",null,"0.75×2m","钢架结构","个",14]
[32,"多功能制丸机",null,"ZW-200","5-50","台",1]
[33,"小型槽形混合机",null,null,"小型槽形混合机","台",1]
[34,"小型干粉混合机",null,null,"小型干粉混合机","台",1]
[35,"小型压片机",null,"TDP-1.5T","外观580*450*625毫米，3600片/时","台",1]
[36,"手工胶囊填充板、定量数片板",null,null,"1#","个",1]
[37,"小型胶囊灌装机",null,"WJP-200A","12000粒/时","台",1]
[38,"电吹风",null,null,"1.5 KW","个",5]
[39,"调温万用电炉",null,"DK-98-1","1KW~1.5KW","台",10]
[40,"层析缸",null,null,"15×5×15","个",6]
[41,"紫外灯",null,"WD-9403E","254,365nm","个",1]
[42,"循环水真空泵",null,"SHE-Ⅲ",null,"台",2]
["小计"]
["二、无机化学实验室"]
[1,"电子天平",null,"BL310","310g(0.01g)","台",2]
[2,"调温万用电炉",null,"DK-98-1","1KW~1.5KW","个",10]
[3,"电吹风",null,null,"1.5 KW","个",2]
[4,"电导率仪",null,"DDS-11At",null,"台",2]
[5,"分光光度计",null,722,"波长驱动：手动\n波长范围(722)：325-1000nm\n波长准确度：±2nm\n波长重复性：≤1nm\n光谱带宽：5nm\n透色比准确度：±1%T\n透色比重复性：≤±0.5%T\n透色比范围：0.0-100%T\n吸光度范围：-0.097-2.000A\n浓度显示范围：0-1999\n杂散光：0.5%T@360nm\n稳定性：≤0.5%T/min\n可与PC联机","台",2]
[6,"磁力搅拌器",null,"JB-1B",null,"台",10]
[7,"真空保温杯",{"$nulls":3},"个",10]
["小计"]
["三、有机化学实验室"]
[1,"旋转蒸发仪",null,"RE52-AA","自动升降，温度数显，电子调速","台",1]
[2,"紫外灯",null,"WD-9403E","254,365(nm)","个",1]
[3,"离心机",null,null,"4000转每分20ml×12","台",2]
[4,"超声波清洗仪",null,"KQ2200DB",null,"台",1]
[5,"显微熔点测定仪",null,"XT3A","50×，10×，最小分度值1℃ 自动控温50-300℃  ","台",1]
[6,"旋光仪",null,"WZZ-1S","测量范围：-45°～+45° \n最小读数值：0.001° \n准确度：±（0.01°+测量值×0.05%） \n重复性（最大偏差）：≤0.002° \n可测样品最低透过率：1% ","台",1]
[7,"电子天平",null,"BL310","310g(0.01g)","台",1]
[8,"调温万用电炉",null,"DK-98-1","1KW~1.5KW","台",10]
[9,"电吹风",null,null,"1.5 KW","个",2]
[10,"水浴锅",null,"DK-2000-IIIL","数显智能型单列双孔","个",5]
["小计"]
["四、分析化学实验室"]
[1,"电子天平",null,"BS210S","0.1mg","台",6]
[2,"水浴锅",null,"DK-2000-IIIL","数显智能型 单列双孔","台",5]
[3,"离心机",null,"DL-8000B-C3号","角式 10ml×12","台",5]
[4,"铂丝",null,null,"0.1mm","克",2]
[5,"调温万用电炉",null,"DK-98-1","1KW~1.5KW","台",10]
[6,"电吹风",null,null,"1.5KW","个",2]
["小计"]
["五、仪器分析实验室"]
[1,"器皿柜",null,null,"2×0.9 ×0.45m","个",1]
[2,"水浴锅",null,"DK-2000-IIIL","数显智能型、单列双孔","台",1]
[3,"电吹风",null,null,"1.5KW","个",1]
["小计"]
["总计"]