{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":60,"n_cols":10,"rows_kept":60,"merged":[[0,0,0,9],[1,0,1,9],[30,0,30,9],[59,0,59,9]],"flags":["formulas_cached_only"]}
["安康学院外语系语言实验室仪器设备招标采购清单"]
["一、数字语言实验室Ⅰ                                  "]
["序号","仪器名称","品牌","参考型号","规    格","单位","数量","单价(元）","金额(元）","备注"]
[1,"多媒体语音网卡",null,"LBD306F","1000M标准网络接口（RJ-45），频率响应40～10000Hz（±2dB），语音传输无断裂、无延迟，失真度0.5%，信噪比70dB（A计权），可负载128台终端，支持45路并发视频流（码流4Mbps），广播延迟5.2ms，视频广播延迟0ms；","块",1]
[2,"多媒体控制平台",null,"LBD2003E-1","能接入并调控多种外围设备（DVD、卡座、功放等），2路VGA输入、6路VGA输出、2路音视频输入、4路音视频输出，支持双显显卡","台",1]
[3,"系统管理软件",null,"LBD2002-NVS","包括听说教学系统、快速阅读系统、小班教学系统、综合教学系统、口译教学系统、视频点播系统、自主录音系统、口译训练系统、考试系统、高信度阅卷系统、备课系统、专业资源库系统、智能化组卷系统、题库管理系统","套",1]
[4,"教师耳机",null,"LBD409H-T","头戴式耳机，带音量调节和话咪开关","个",1]
[6,"                                                                                                                                       多媒体网络交换主机",null,"                          LBD309A","自主研发1000M网络交换机，采用异步网络的同步传输技术，确保音频、视频、图像等多媒体信息实时高保真传输，具有1个1000M接口,16个100M接口","                         台",1]
[7,"多媒体网络交换分机",null,"LBD309B"," 自主研发ATM网、以太网两网合一交换机，配套视频广播协议，实现语言教学、考试、上网、自学等。16个100M接口，数据转发无延迟、无断裂，保证音视频的实时传输","台",3]
[8,"语言学习终端",null,"LBD2002-NVC","自主研发嵌入式终端，采用专业解码芯片和处理器，可提供系统所需的各种接口，支持标准鼠标键盘和显示器，支持USB设备，支持网页浏览，支持PDF、WORD、EXCEL等文件浏览。可进行音频、文本、图片及视频的点播学习，支持高清视频（1080P）点播；终端支持的音视频格式包括MP3、MP4、WMA、WAV、MPG、MPEG、AVI、DAT、VOB等；4个USB接口、VGA接口、RJ45网络接口、3个3.5mm音频接口，学生收听语音时,终端有自主变速不变调功能（范围±30％）","个",38]
[9,"键盘",null,"M315","可进行语言学习操作及字符输入","个",38]
[10,"鼠标",null,"K6000","光电鼠标,PS/2接口","个",38]
[11,"学生耳机",null,"LC-EP16N1","头戴式耳机，立体声/带话咪，动圈式工作方式","个",38]
[12,"线材",null,"国产","VGA线/电缆线（电源线）/网线","位",38]
[13,"杂配件",null,"国产","多功能插板/插座/线槽等","位",38]
[14,"操作主机",null,"方正","Intel酷睿双核E7400/华硕主板/2*1G DDR2内存/4*SATA 320G硬盘/512M双头显卡/DVD刻录机/1.44软驱/键盘/光电鼠标/机箱电源/可选硬盘保护卡","台",1]
[15,"教师位显示器",null,"19\"液晶","19\"液晶显示器（长城 联想 LG 方正AOC）","台",2]
[16,"学生显示器",null,"17\"液晶","17\"液晶显示器（长城 联想 LG 方正AOC）","台",38]
[17,"视频展示台",null,"鸿合6100","1/4英寸专业数码CCD镜头，80万 象素,正负片\n,15倍光学放大，8～10倍电子放大 信噪比>48dB\n 带VGA输出 1024*768，60Hz","台",1]
[18,"音箱",null,"湖山R50","50W+50W，阻抗8欧姆，自带音箱支架","台",1]
[19,"功放",null,"湖山XYIOO","额定功率60w+60w(最大功率350w)，阻抗8欧姆，频率响应20-20KHz","台",1]
[20,"DVD",null,"奇声","频率特性：20Hz-20KHz(±1dB),信噪比>90dB,总谐波失真<0.01%,电源：110V~240V,交流电压：50/60Hz,功耗：14W,支持USB设备及话筒输入","台",1]
[21,"投影机",null,"日立HCP-3000X","LCD 2600流明、分辨率1024*768 对比度600:1","台",1]
[22,"幕布",null,"三叶","100寸电动","副",1]
[23,"分配器",null,"蓝宝","一分四","个",1]
[24,"教师控制台 ",null,"LBS-J02A","240×80（cm）高密度板材.含升降靠背转椅","台",1]
[25,"学生桌/凳子",null,"LBS-X02SVA","130×60（cm）学生桌高密度板材. 凳子钢木结构","张",19]
[26,"其他附材",null,"国产","PVC、贴号、空开等","批",1]
[27,"静电地板",null,"双奇","钢制地板，钢板厚度不少于1.2毫米，国家免检产品。","M2",70]
["小计"]
["二、数字语言实验室II                                  "]
[1,"多媒体语音网卡",null,"LBD306F","1000M标准网络接口（RJ-45），频率响应40～10000Hz（±2dB），语音传输无断裂、无延迟，失真度0.5%，信噪比70dB（A计权），可负载128台终端，支持45路并发视频流（码流4Mbps），广播延迟5.2ms，视频广播延迟0ms；","块",1]
[2,"多媒体控制平台",null,"LBD2003E-1","能接入并调控多种外围设备（DVD、卡座、功放等），2路VGA输入、6路VGA输出、2路音视频输入、4路音视频输出，支持双显显卡","台",1]
[3,"系统管理软件",null,"LBD2002-NVS","包括听说教学系统、快速阅读系统、小班教学系统、综合教学系统、口译教学系统、视频点播系统、自主录音系统、口译训练系统、考试系统、高信度阅卷系统、备课系统、专业资源库系统、智能化组卷系统、题库管理系统","套",1]
[4,"教师耳机",null,"LBD409H-T","头戴式耳机，带音量调节和话咪开关","个",1]
[6,"                                                                                                                                       多媒体网络交换主机",null,"                          LBD309A","自主研发1000M网络交换机，采用异步网络的同步传输技术，确保音频、视频、图像等多媒体信息实时高保真传输，具有1个1000M接口,16个100M接口","                         台",1]
[7,"多媒体网络交换分机",null,"LBD309B"," 自主研发ATM网、以太网两网合一交换机，配套视频广播协议，实现语言教学、考试、上网、自学等。16个100M接口，数据转发无延迟、无断裂，保证音视频的实时传输","台",3]
[8,"语言学习终端",null,"LBD2002-NVC","自主研发嵌入式终端，采用专业解码芯片和处理器，可提供系统所需的各种接口，支持标准鼠标键盘和显示器，支持USB设备，支持网页浏览，支持PDF、WORD、EXCEL等文件浏览。可进行音频、文本、图片及视频的点播学习，支持高清视频（1080P）点播；终端支持的音视频格式包括MP3、MP4、WMA、WAV、MPG、MPEG、AVI、DAT、VOB等；4个USB接口、VGA接口、RJ45网络接口、3个3.5mm音频接口，学生收听语音时,终端有自主变速不变调功能（范围±30％）","个",42]
[9,"键盘",null,"M315","可进行语言学习操作及字符输入","个",42]
[10,"鼠标",null,"K6000","光电鼠标,PS/2接口","个",42]
[11,"学生耳机",null,"LC-EP16N1","头戴式耳机，立体声/带话咪，动圈式工作方式","个",42]
[12,"线材",null,"国产","VGA线/电缆线（电源线）/网线","位",42]
[13,"杂配件",null,"国产","多功能插板/插座/线槽等","位",42]
[14,"操作主机",null,"方正","Intel酷睿双核E7400/华硕主板/2*1G DDR2内存/4*SATA 320G硬盘/512M双头显卡/DVD刻录机/1.44软驱/键盘/光电鼠标/机箱电源/可选硬盘保护卡","台",1]
[15,"教师位显示器",null,"19\"液晶","19\"液晶显示器（长城 联想 LG 方正AOC）","台",2]
[16,"学生显示器",null,"17\"液晶","17\"液晶显示器（长城 联想 LG 方正 AOC）","台",42]
[17,"视频展示台",null,"鸿合6100","1/4英寸专业数码CCD镜头，80万 象素,正负片\n,15倍光学放大，8～10倍电子放大 信噪比>48dB\n 带VGA输出 1024*768，60Hz","台",1]
[18,"音箱",null,"湖山R50","50W+50W，阻抗8欧姆，自带音箱支架","台",1]
[19,"功放",null,"湖山XYIOO","额定功率60w+60w(最大功率350w)，阻抗8欧姆，频率响应20-20KHz","台",1]
[20,"DVD",null,"奇声","频率特性：20Hz-20KHz(±1dB),信噪比>90dB,总谐波失真<0.01%,电源：110V~240V,交流电压：50/60Hz,功耗：14W,支持USB设备及话筒输入","台",1]
[21,"投影机",null,"日立HCP-3000X","LCD 2600流明、分辨率1024*768 对比度600:1","台",1]
[22,"幕布",null,"三叶","100寸电动","副",1]
[23,"分配器",null,"蓝宝","一分四","个",1]
[24,"教师控制台 ",null,"LBS-J02A","240×80（cm）高密度板材.含升降靠背转椅","台",1]
[25,"学生桌/凳子",null,"LBS-X02SVA","130×60（cm）学生桌高密度板材. 凳子钢木结构","张",21]
[26,"其他附材",null,"国产","PVC、贴号、空开等","批",1]
[27,"静电地板",null,"双奇","钢制地板，钢板厚度不少于1.2毫米，国家免检产品。","M2",65]
["小计"]
["总计"]
["备注：以上产品（系统）须符合国家教育技术协会《数字语言学习系统技术规范》A级或甲类标准和《语言学习网络平台规范》。"]