{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["sheet1"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"sheet1","index":0,"n_rows":9,"n_cols":9,"rows_kept":9,"merged":[[0,0,0,8]],"flags":["formulas_cached_only"]}
["安康学院蚕桑重点实验室仪器设备采购清单"]
[]
["序号","设备名称","品牌型号","规格","单位","数量","单价(元)","金额(元)","备注"]
[1,"电转化仪",null,"电压 200-2,500V \n电容 l0μF，2,500V电脉冲放电 \n充电时间 <8秒 \n时间参数 一般设定5ms／为一个样本，抗阻3.3KΩ\n接口 RS232\n附电击杯(1MM,2MM,4MM) ","台",1]
[2,"彩通色彩检测仪","PANTONE(潘通) GEB103 -2型  ","CMYK 四色配色手册（最新版） ","台",1]
[3,"对色灯箱","PANTONE(潘通) CAC-600-五光源","电压: 220V /110V \n一  D65 国际标准人工日光光源 2 支 20W/支 6500K \n二  84 欧洲、日本商用光源 2 支 18W/支 4000K \n三  UV 紫外光源 1 支 20W/ 支 \n四  F 黄光源、比色参考光源 4 只 40W/只 2700K \n五  CWF 美国商店光源 2 支 20W/支 4200K ","台",1]
[4,"GPS测量仪","麦哲伦\n探险者600","内置全国地图,定位精度<7米,黑色","台",1]
[5,"面积测量仪","麦哲伦\n探险者210","内置全国地图,面积测量,定位精度<7米,黄色","台",1]
[null,"合计"]